GENERAL NOTES |  |  |  |  |  |  |
SUMMARY OF XSF FLAGS |  |
XSF 1 | - | Auto introduce Pedestrian 1 | & 2 |
GENERAL OPERATION |  |
Expire B ECO when transitioning B -> C. |
Use B Special All Red when transitioning B -> C. |
PEDESTRIAN GROUP OPERATION |
Pedestrian 1 |  |
P1 demands A. |  |
P1 introduces at the start of A. |
P1 auto introduces at the start of A if XSF 1 is set. |
Pedestrian 2 |  |
P2 demands A. |  |
P2 introduces at the start of A. |
P2 auto introduces at the start of A if XSF 1 is set. |
Pedestrian 3 |  |
P3 demands B. |  |
P3 introduces at the start of B. |
Pedestrian 4 |  |
P4 demands B. |  |
P4 introduces at the start of B. |
DETECTOR OPERATION |  |
Detectors 9 & 10 |  |
Clear calls for B from Detectors 9 & 10 during Signal Group 3 green & yellow. |
Detectors 11 & 12 |  |
Clear calls for B from Detectors 11 & 12 during Signal Group 5 green & yellow. |
Detector 13 |  |
Clear calls for B from Detector 13 during Signal Group 4 green & yellow. |
Detector 14 |  |
Clear calls for B from Detector 14 during Signal Group 4 green. |
Detector 14 places non-locking calls for C when its presence time expires during B green.
Clear calls for C from Detector 14 during Signal Group 7 green. |
Detector 15 |  |
Clear calls for B from Detector 15 during Signal Group 6 green & yellow. |
Detector 16 |  |
Clear calls for B from Detector 16 during Signal Group 6 green. |
Detector 16 places non-locking calls for C when its presence time expires during B green.
Clear calls for C from Detector 16 during Signal Group 8 green. |