|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 3/1
SITE NAME | PRINCES HIGHWAY EAST NR SERVICE STREET | SITE NO. | 5655
PEDESTRIAN OPERATION
PELICAN OPERATION
OPERATION OF SG1 & SG2 WHEN CROSSING IS OPERATING AS A PELICAN POS |
SG1 closes down to introduce P1 according to the notes on pages 2 and 4 of this Operation Specification. When it closes down it uses the yellow and all red times as described in note 2 on page 4.
SG2 closes down to introduce P2 according to the notes on pages 2 and 4 of this Operation Specification. When it closes down it uses the yellow and all red times as described in note 2 on page 4.
SG1 remains red during SG1 all red, P1 walk and P1 clearance 1. |  |
SG2 remains red during SG2 all red, P2 walk and P2 clearance 1. |  |
At the start of P1 clearance 2, SG1 goes to flashing yellow mode. |  |
At the start of P2 clearance 2, SG2 goes to flashing yellow mode. |  |
SG1 remains in flashing yellow mode during P1 clearance 2 and P1 solid DONT WALK |
SG2 remains in flashing yellow mode during P2 clearance 2 and P2 solid DONT WALK |
SG1 goes green at the end of P1 solid DONT WALK |  |  |  |  |
SG2 goes green at the end of P2 solid DONT WALK |  |  |  |  |
The flash rate of SG1 & SG2 when in flashing yellow mode is as follows: |  |  |
- SG1 & SG2 yellow is on for 0.5 seconds |  |  |  |  |
- SG1 & SG2 yellow is off for 0.5 seconds |  |  |  |  |
OPERATION OF SG1 & SG2 WHEN CROSSING IS OPERATING AS A NORMAL POS |
When the POS detector is on, the operation of the crossing changes to that of a normal pedestrian crossing and SG1 & SG2 operate as described below.
SG1 closes down to introduce P1 according to the notes on pages 2 and 4 of this Operation Specification. When it closes down it uses the yellow and all red times as described in note 2 on page 4.
SG2 closes down to introduce P2 according to the notes on pages 2 and 4 of this Operation Specification. When it closes down it uses the yellow and all red times as described in note 2 on page 4.
SG1 remains red during SG1 all red, P1 walk, P1 clearance 1, P1 clearance 2 and P1 solid DONT WALK |
SG2 remains red during SG2 all red, P2 walk, P2 clearance 1, P2 clearance 2 and P2 solid DONT WALK |
SG1 goes green at the end of P1 solid DONT WALK. |  |  |
SG2 goes green at the end of P2 solid DONT WALK. |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) | DATE | 30/06/15