|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 7 |  |
SITE NAME | PHE BTW LYONS ST & HOOD ST |  | SITE NO. | 5611 |
FLEXILINK OPERATION |
PHASE SEQUENCES |
No | PHASE SEQUENCE |  | NOTES: |
1 (No Y+) | ABCDEF (Only ABC run) |  | 1. All phases must be specified in the phase sequence |
2 (Y+) | ABCDEF |  | 2. Only specify phase sequence 2 if it is different from phase sequence 1. |
LOOK AHEADS & RELEASES |
PHASE SEQUENCE 1 |  | PHASE SEQUENCE 2 |  |
PHASE | LOOK AHEAD* | RELEASE |  | PHASE | LOOK AHEAD* | RELEASE |  |
A | No | No |  | A | No | No |  |
B | No | No |  | B | No | No |  |
C | No | No |  | C | No | No |  |
D | No | No |  | D | No | No |  |
E | No | No |  | E | No | No |  |
F | No | No |  | F | No | No |  |
G | No | No |  | G | No | No |  |
* Specify the phases to which look ahead is permitted, eg. Yes (to E, F, G, A) |
INHIBIT PHASES |
The following phases can be inhibited in flexilink by setting the call pulse one step before the call pulse of the next phase in sequence | B, E |
PULSE STEP LENGTH |
| One Second |  | P | Two Second |
MASTERLINK & FLEXILINK SPECIAL FLAGS |
FLAG | FUNCTION |
Y- | Flexi | The site will operate in flexilink mode if the signal is continuously sent (C) or is used as an offset (eg 25) |  |
Y- | Master |  |
Y+ | Flexi | Double phasing, ie. Run ABCDEF |
Z- | Flexi |  |
Z- | Master |  |
Z+ | Flexi |  |
Z+ | Master |  |
R- | Flexi | Queuing Feature (refer notes on page 6) |
R+ | Flexi | Queuing Feature (refer notes on page 6) |
Q- | Flexi | Queuing Feature (refer notes on page 6) |
Q+ | Flexi | Queuing Feature (refer notes on page 6) |
DESIGNED BY: | [REDACTED] |  | DATE | 1/07/05 |
G:\TMC Opsheets\Pending\[5611.htm]Flexi |  |