|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 4 |  |
SITE NAME | PRINCES HIGHWAY EAST NR SERVICE STREET |  | SITE NO. | 5655 |
CONTROLLER TIMESETTINGS - 1 |
PHASE TIMESETTINGS | Front Panel Command: Phase No.Timesetting No (e.g. 1.6 accesses A phase maximum extension green) |
DESCRIPTION | Timesetting No | PHASE |
A (1) | B (2) | C (3) | D (4) | E (5) | F (6) | G (7) |
RED / YELLOW | 1 | - | - | - |  |  |  |  |
LATE START | 2 | - | - | - |  |  |  |  |
MINIMUM GREEN (1) | 3 | 3.0 | 0.0 | 3.0 |  |  |  |  |
INCREMENT | 4 | - | - | - |  |  |  |  |
MAXIMUM INITIAL GREEN | 5 | - | - | - |  |  |  |  |
MAXIMUM EXTENSION GREEN (4) | 6 | 40 | - | - |  |  |  |  |
EARLY CUT OFF | 7 | - | - | - |  |  |  |  |
YELLOW (2) | 8 | 3.5 | 3.5 | 3.5 |  |  |  |  |
ALL RED (2) | 9 | 0.0 | 2.0 | 0.0 |  |  |  |  |
SPECIAL ALL RED | 10 | - | - | - |  |  |  |  |
GAP 1 (3) | 11 | 2.5 | - | - |  |  |  |  |
GAP 2 (3) | 12 | 2.5 | - | - |  |  |  |  |
GAP 3 | 13 | - | - | - |  |  |  |  |
GAP 4 | 14 | - | - | - |  |  |  |  |
HEADWAY 1 | 15 | 0.6 | - | - |  |  |  |  |
HEADWAY 2 | 16 | 0.6 | - | - |  |  |  |  |
HEADWAY 3 | 17 | - | - | - |  |  |  |  |
HEADWAY 4 | 18 | - | - | - |  |  |  |  |
WASTE 1 | 19 | 7 | - | - |  |  |  |  |
WASTE 2 | 20 | 7 | - | - |  |  |  |  |
WASTE 3 | 21 | - | - | - |  |  |  |  |
WASTE 4 | 22 | - | - | - |  |  |  |  |
1. For SG1 and SG2 minimum green in VA mode, refer Special Purpose Timesetting 17 & 21. |  |  |  |  |
For SG1 and SG2 minimum green in link mode, refer Special Purpose Timesetting 20 & 22. |  |
2. SG1 can close down during B, SG2 can close down during A, B or C |  |
SG1 and SG2 use the yellow time of the phase they close down in, but use the all red times specified in Special Movement Timesettings 1& 2. |
3. SG1 and SG2 use the gap, headway and waste times specified in A timesettings. |  |
4. A maximum extension green is used only in VA mode. |  |
PEDESTRIAN TIMESETTINGS | Front Panel Command: Pedestrian No.Timesetting No (e.g. 18.2 accesses P2 walk) |  |
DESCRIPTION | Timesetting No | PEDESTRIAN |
P1 (17) | P2 (18) | P3 (19) | P4 (20) | P5 (21) | P6 (22) | P7 (23) | P8 (24) |
DELAY | 1 | - | - |  |  |  |  |  |  |
WALK* | 2 | 10 | 10 |  |  |  |  |  |  |
CLEARANCE 1 | 3 | 3 | 3 |  |  |  |  |  |  |
CLEARANCE 2 | 4 | 6 | 6 |  |  |  |  |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) |  | DATE | 30/06/15 |