GENERAL NOTES |  |  |  |  |  |  |  |
SUMMARY OF XSF FLAGS |
(Communications Operation of XSF flags is required) |
XSF1 | - | Allow late introduction of P1 in A (Masterlink only). |
XSF2 | - | Allow late introduction of P2 in A (Masterlink only). |
XSF5 | - | Special maximum for SG5 in D via Special Purpose Timesetting No. 9. |
XSF6 | - | Special maximum for SG6 in D via Special Purpose Timesetting No. 10. |
XSF7 | - | Special maximum for SG7 in B via Special Purpose Timesetting No. 11. |
XSF8 | - | Special maximum for SG8 in B via Special Purpose Timesetting No. 12. |
GENERAL OPERATION |
● | Substitute Special Purpose Timesetting No. 13 for P1 walk when P1 is demanded via detector 16.
● | Substitute Special Purpose Timesetting No. 14 for P2 walk when P2 is demanded via detector 17.
● | Substitute Special Purpose Timesetting No. 15 for P3 walk when P3 is demanded via detector 18.
● | Substitute Special Purpose Timesetting No. 16 for P4 walk when P4 is demanded via detector 19.
PEDESTRIAN GROUP OPERATION |
Pedestrian 1 |  |
● | P1 calls A. |
● | P1 can introduce any time in D3 and at the start of A and overlap from D3 -> A. |
● | P1 can introduce any time in A when XSF1 is set (masterlink only). |
Pedestrian 2 |  |
● | P2 calls A. |
● | P2 can introduce any time in D2 and at the start of A and overlap from D2 -> A. |
● | P2 can introduce any time in A when XSF2 is set (masterlink only). |
Pedestrian 3 |  |
● | P3 calls C. |
● | P3 can introduce any time in B2 and at the start of C and overlap from B2 -> C. |
Pedestrian 4 |  |
● | P4 calls C. |
● | P4 can introduce any time in B3 and at the start of C and overlap from B3 -> C. |
DETECTOR OPERATION |
● | Detector 16 is a wheel chair input. Detector 16 places demand for P1 when its presence time expires.
● | Detector 17 is a wheel chair input. Detector 17 places demand for P2 when its presence time expires.
● | Detector 18 is a wheel chair input. Detector 18 places demand for P3 when its presence time expires.
● | Detector 19 is a wheel chair input. Detector 19 places demand for P4 when its presence time expires.