|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  | PAGE 3/1
SITE NAME | PHE BTW LYONS ST & HOOD ST | SITE NO. | 5611
PEDESTRIAN OPERATION
PELICAN OPERATION
OPERATION OF SG1 & SG2 WHEN CROSSING IS OPERATING AS A PELICAN POS |
SG1 & SG2 close down to introduce P1 according to the notes on pages 2 and 4 of this Operation Specification.
When closing down SG1 & SG2, they use the yellow and all red times as described in note 2 on page 4. |
SG1 & SG2 remain red during SG1 & SG2 all red, P1 walk and P1 clearance 1. |  |
At the start of P1 clearance 2, SG1 & SG2 go to flashing yellow mode. |  |
SG1 & SG2 remain in flashing yellow mode during P1 clearance 2 and P1 solid DONT WALK |
SG1 & SG2 go green at the end of P1 solid DONT WALK |  |  |  |  |
The flash rate of SG1 & SG2 when in flashing yellow mode is as follows: |  |  |
- SG1 & SG2 yellow is on for 0.5 seconds |  |  |  |  |
- SG1 & SG2 yellow is off for 0.5 seconds |  |  |  |  |
OPERATION OF SG1 & SG2 WHEN CROSSING IS OPERATING AS A NORMAL POS |
When detector 6 is on, the operation of the crossing changes to that of a normal pedestrian crossing and |
SG1 & SG2 operate as described below. |  |  |
SG1 & SG2 close down to introduce P1 according to the notes on pages 2 and 4 of this Operation Specification.
When closing down SG1 & SG2, they use the yellow and all red times as described in note 2 on page 4.
SG1 & SG2 remain red during SG1 & SG2 all red, P1 walk, P1 clearance 1, P1 clearance 2 and |
P1 solid DONT WALK |  |
SG1 & SG2 go green at the end of P1 solid DONT WALK. |  |  |
DESIGNED BY: | [REDACTED] | DATE | 1/07/05
G:\TMC Opsheets\Pending\[5611.htm]PELICAN Notes