|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 9 |  |
SITE NAME | PRINCES HIGHWAY EAST/RAYMOND ST |  | SITE NO. | 5603 |
FLEXILINK OPERATION |
PHASE SEQUENCES |
No | PHASE SEQUENCE |  | NOTES: |
1 (No Y+) | AB |  | 1. All phases must be specified in the phase sequence |
2 (Y+) |  |  | 2. Only specify phase sequence 2 if it is different from phase sequence 1. |
LOOK AHEADS & RELEASES |
PHASE SEQUENCE 1 |  | PHASE SEQUENCE 2 |  |
PHASE | LOOK AHEAD* | RELEASE |  | PHASE | LOOK AHEAD* | RELEASE |  |
A | No | R- |  | A |  |  |  |
B | No | R+ |  | B |  |  |  |
C |  |  |  | C |  |  |  |
D |  |  |  | D |  |  |  |
E |  |  |  | E |  |  |  |
F |  |  |  | F |  |  |  |
G |  |  |  | G |  |  |  |
* Specify the phases to which look ahead is permitted, eg. Yes (to E, F, G, A) |
INHIBIT PHASES |
The following phases can be inhibited in flexilink by setting the call pulse one step before the call pulse of the next phase in sequence | - |
PULSE STEP LENGTH |
| One Second |  | P | Two Second |
MASTERLINK & FLEXILINK SPECIAL FLAGS |
FLAG | FUNCTION |
Y- | Flexi | The site will operate in flexilink mode if the signal is continuously sent (C) or is used as an offset (eg 25) |  |
Y- | Master |  |
Y+ | Flexi |  |
Z- | Flexi |
Auto introduction of P1 & P2
Z- | Master |
Z+ | Flexi |
Auto introduction of P3 & P4
Z+ | Master |
R- | Flexi | A Release pulse |
R+ | Flexi | B Release pulse |
Q- | Flexi |  |
Q+ | Flexi | P1, P2, P3 & P4 Walk time substitutions (Refer Special Purpose Timesettings No. 9, 10, 11, & 12) |
DESIGNED BY: | [REDACTED] [REDACTED] |  | DATE | 20-Apr-04 |
G:\TCCC Opsheets\Pending\[5603.htm]Flexi |