GENERAL NOTES |  |  |  |  |
SUMMARY OF XSF FLAGS |
(Communications Operation of XSF flags is required) |
XSF1 | - | Allow automatic introduction of P1 in C. |
GENERAL OPERATION |
Clear demands for B and D during SG5 green and yellow. |
Clear demands for C via detector 5 during SG5 green and yellow in D.
If transitioning from B -> A, substitute D yellow for B yellow. |
PEDESTRIAN GROUP OPERATION |
Pedestrian 1 |  |
P1 calls C. |  |
P1 can introduce at the start of C. |
P1 can auto introduce at the start C if XSF1 is set. |