|  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 12 |  |  |  |  |  |  |
SITE NAME | PRINCES HIGHWAY EAST / MACALISTER STREET | SITE NO. | 5607 |
FLEXILINK PLAN DATA |  |
Front Panel Command: E.Plan No.Plan Item No (e.g. E.2.10 accesses Plan 2 Y- flag) |  |
PLAN ITEM No | DESCRIPTION | Plan No |  |
0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 |  |
0 | CL | 0 |  |  |  |  |  |  |  |  |  |  |  |
1 | Call A |  |  |  |  |  |  |  |  |  |  |  |  |
2 | Call B |  |  |  |  |  |  |  |  |  |  |  |  |
3 | Call C |  |  |  |  |  |  |  |  |  |  |  |  |
4 | Call D |  |  |  |  |  |  |  |  |  |  |  |  |
5 | Call E |  |  |  |  |  |  |  |  |  |  |  |  |
6 | Call F |  |  |  |  |  |  |  |  |  |  |  |  |
7 | Call G |  |  |  |  |  |  |  |  |  |  |  |  |
8 | R- flag |  |  |  |  |  |  |  |  |  |  |  |  |
9 | R+ flag |  |  |  |  |  |  |  |  |  |  |  |  |
10 | Y- flag |  |  |  |  |  |  |  |  |  |  |  |  |
11 | Y+ flag |  |  |  |  |  |  |  |  |  |  |  |  |
12 | Z- flag |  |  |  |  |  |  |  |  |  |  |  |
13 | Z+ flag |  |  |  |  |  |  |  |  |  |  |  |
14 | Q- flag |  |  |  |  |  |  |  |  |  |  |  |
15 | Q+ flag |  |  |  |  |  |  |  |  |  |  |  |
16 | XSF (9-16)* |  |  |  |  |  |  |  |  |  |  |  |
17 | XSF (1-8)* |  |  |  |  |  |  |  |  |  |  |  |
* A 2 digit hexadecimal number which signifies which XSF bits are set; e.g. A0 signifies bits 14 & 16 are set. |
(Refer to SCATS Handbook Chapter 22 for SCATS 5. For SCATS 6 operation, refer to pages 20 - 22. |
Notes: |
1. If the controller is off line, enter 254 via the front panel for N = signal not sent |
2. If the controller is off line, enter 255 via the front panel for C = signal continuously sent |
DESIGNED BY: | [REDACTED] [REDACTED] (CPG) | DATE | 18/08/10 |
G:\TMC Opsheets\Pending\[5607.htm]Flexi Plan Data |  |