|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 6 |  |
SITE NAME | PHE / MAFFRA - SALE ROAD |  | SITE NO. | 5610 |
CONTROLLER TIMESETTINGS - 1 |
PHASE TIMESETTINGS | Front Panel Command: Phase No.Timesetting No (eg 3.2 accesses C phase late start) |
DESCRIPTION | Timesetting No | PHASE |
A (1) | B (2) | C (3) | D (4) | E (5) | F (6) | G (7) |
RED / YELLOW | 1 | - | - | - | - | - | - | - |
LATE START | 2 | - | - | - | - |  |  |  |
MINIMUM GREEN | 3 | 10 | 6 | 6 | 6 |  |  |  |
INCREMENT | 4 | - | - | - | - |  |  |  |
MAXIMUM INITIAL GREEN* | 5 | - | - | - | - |  |  |  |
MAXIMUM EXTENSION GREEN | 6 | 40 | 10 | 20 | 10 |  |  |  |
EARLY CUT OFF | 7 |  |  |  |  |  |  |  |
YELLOW | 8 | 4.5 | 4.5 | 3.0 | 3.0 |  |  |  |
ALL RED | 9 | 1.5 | 2.0 | 2.5 | 2.0 |  |  |  |
SPECIAL ALL RED | 10 | - | - | - | - |  |  |  |
GAP 1 | 11 | 3.0 | 2.5 | 2.5 | 2.5 |  |  |  |
GAP 2 | 12 | 3.0 | - | - | - |  |  |  |
GAP 3 | 13 | - | - | - | - |  |  |  |
GAP 4 | 14 | - | - | - | - |  |  |  |
HEADWAY 1 | 15 | 0.6 | 1.2 | 1.2 | 1.2 |  |  |  |
HEADWAY 2 | 16 | 1.2 | - | - | - |  |  |  |
HEADWAY 3 | 17 | - | - | - | - |  |  |  |
HEADWAY 4 | 18 | - | - | - | - |  |  |  |
WASTE 1 | 19 | 10 | 7 | 7 | 7 |  |  |  |
WASTE 2 | 20 | 10 | - | - | - |  |  |  |
WASTE 3 | 21 | - | - | - | - |  |  |  |
WASTE 4 | 22 | - | - | - | - |  |  |  |
* Maximum Initial Green = Minimum Green + V.I.G. |  |
PEDESTRIAN TIMESETTINGS | Front Panel Command: Pedestrian No.Timesetting No (eg 18.2 accesses P2 walk) |  |
DESCRIPTION | Timesetting No | PEDESTRIAN |
P1 (17) | P2 (18) | P3 (19) | P4 (20) | P5 (21) | P6 (22) | P7 (23) | P8 (24) |
DELAY | 1 | - | - | - | - | - | - | - | - |
WALK* | 2 | 13.0 |  |  |  |  |  |  |  |
CLEARANCE 1 | 3 | 6.0 |  |  |  |  |  |  |  |
CLEARANCE 2 | 4 | 1.0 |  |  |  |  |  |  |  |
* Minimum walk time - used in Isolated and Flexilink operation |  |
For walk times in Masterlink operation, refer to slot data. |  |
DESIGNED BY: | [REDACTED] [REDACTED] |  | DATE | 23-Apr-12 |
G:\TMC Opsheets\Pending\[5610.htm]Controller 1 |