|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 6 |  |
SITE NAME | PRINCES HIGHWAY EAST NR SERVICE STREET |  | SITE NO. | 5655 |
CONTROLLER TIMESETTINGS - 3 |
PRESENCE TIMESETTINGS | Front Panel Command: D.Detector No (e.g. D.7 accesses Presence time for detector 7) |  |
DETECTOR No | TIMESETTING (Range: 0-10) |  |
1 |  |  |
2 |  |  |
3 |  |  |
4 |  |  |
5 | 6.0 |  |
6 | 6.0 |  |
7 | 6.0 |  |
8 | 6.0 |  |
9 |  |  |
10 |  |  |
11 |  |  |
12 |  |  |
QUEUING FEATURE |
APPROACH 1: |
- If XSF9 (Masterlink) or R- (Flexilink) is set, and the presence time for detector 5 and/or detector 6 is expired in B, and there is a demand for P1, expire approach 1 |
APPROACH 2: |
- If XSF10 (Masterlink) or R+ (Flexilink) is set, and the presence time for detector 7 and/or detector 8 is expired, and there is a demand for P2 when a special timer (Refer Special Purpose Timesetting No 25) has expired, expire approach 2. The special timer starts when T1 expires. |
DAILY EVENT TIMESETTINGS |  |  |
FUNCTION | TIMESETTING |  |
Daily start time | (Hours) |  |  |
Daily start time | (Minutes) |  |  |
Daily finish time | (Hours) |  |  |
Daily finish time | (Minutes) |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) |  | DATE | 30/06/15 |