|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |
SITE NAME | PRINCES HIGHWAY EAST / MCCULLOCH STREET | SITE NO. | 5659 |  |
DESIGN OF INTERGREEN AND PEDESTRIAN TIMES |  |
INTERGREEN TIMES |  |  |  |  |
PHASE | CLEARANCE DETAILS | LEGAL SPEED | DESIGN SPEED | INTERGREEN |  |  |
GROUP TRANSITION | DISTANCE | YELLOW | RED | YELLOW | RED | TOTAL |
A | 1 | g | P3 | 32.0 | 60 | 60 | 40 | 4.0 | 3.0 | 7.0 |  |  |  |
B | 4 | g | P2 | 21.0 | 60 | 60 | 40 | 4.0 | 2.0 | 6.0 |  |  |  |
C | 4 | g | P2 | 21.0 | 60 | 60 | 40 | 4.0 | 2.0 | 6.0 |  |  |  |
D |  | g |  |  |  |  |  |  |  |  |  |  |  |
E |  | g |  |  |  |  |  |  |  |  |  |  |  |
F |  | g |  |  |  |  |  |  |  |  |  |  |  |
G |  | g |  |  |  |  |  |  |  |  |  |  |  |
| Red times calculated for 40 kph school zone. |  |  |  |  |
PHASE SPECIAL ALL REDS AND SPECIAL MOVEMENT ALL REDS |  |  |  |  |
FROM PHASE | TO PHASE | CLEARANCE DETAILS | DESIGN SPEED | ALL RED | PHASE or S.M. No* |  |  |  |
GROUP TRANSITION | DISTANCE |  |  |  |
B | C | 5 | g | 7 | 17.0 | 40 | 1.5 | B PHASE SPECIAL ALL RED |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
C | B | 7 | g | P4 | 22.0 | 40 | 2.0 | - |  |  |
|  |  | g |  |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
* Specify where the timesetting is stored (the phase special all red or the special movement time setting number) |  |  |  |
PEDESTRIAN TIMES |  |  |
PED | PHASE(S) | WALK | CLEARANCE | MINIMUM SOLID DON'T WALK |  |  |
DISTANCE (m) | TIME | DISTANCE (m) | TIME |
GRAPH | ADOPTED | GRAPH | CL1 | CL2 |
1 | A |  | 16.0 | 15 | 16 | 8.0 | 5 | 6.0 |  | 7.0 |  |  | 7 |
2 | A |  | 15.0 | 15 | 16 | 9.0 | 6 | 6.0 |  | 7.0 |  |  | 10 |
3 | B |  | 14.0 | 8 | 10 | 14.0 | 9 | 10.0 |  | 5.5 |  |  | 6 |
4 | B |  | 14.0 | 8 | 10 | 14.0 | 9 | 10.0 |  | 5.5 |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) | DATE | 30/06/15 |  |