|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 6 |  |
SITE NAME | PHE BTW LYONS ST & HOOD ST |  | SITE NO. | 5611 |
CONTROLLER TIMESETTINGS - 3 |
PRESENCE TIMESETTINGS | Front Panel Command: D.Detector No (eg D.7 accesses Presence time for detector 7) |  |
DETECTOR No | TIMESETTING (Range: 0-10) |  |
1 | 6.0 |  |
2 | 6.0 |  |
3 | 6.0 |  |
4 | 6.0 |  |
5 |  |  |
6 |  |  |
7 |  |  |
8 |  |  |
9 |  |  |
10 |  |  |
11 |  |  |
12 |  |  |
QUEUEING FEATURE |
APPROACH 1: |
- If XSF9 (Masterlink) or R- (Flexilink) is set, and the presence time for detector 1 and/or detector 2 is expired in B, and there is a demand for P1, expire approach 1 |
- If XSF9 (Masterlink) or Q- (Flexilink) is set, and the presence time for detector 1 and/or detector 2 is expired in E, and there is a demand for P1, expire approach 1 |
APPROACH 2: |
- If XSF10 (Masterlink) or R+ (Flexilink) is set, and the presence time for detector 3 and/or detector 4 is expired in B, and there is a demand for P1, expire approach 2 |
- If XSF10 (Masterlink) or Q+ (Flexilink) is set, and the presence time for detector 3 and/or detector 4 is expired in E, and there is a demand for P1, expire approach 2 |
DAILY EVENT TIMESETTINGS |  |  |
FUNCTION | TIMESETTING |  |
Daily start time | (Hours) |  |  |
Daily start time | (Minutes) |  |  |
Daily finish time | (Hours) |  |  |
Daily finish time | (Minutes) |  |  |
DESIGNED BY: | [REDACTED] |  | DATE | 1/07/05 |
G:\TMC Opsheets\Pending\[5611.htm]Controller 3 |