|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 7 |
SITE NAME | PRINCES HIGHWAY EAST / MACALISTER STREET |  | SITE NO. | 5607 |
CONTROLLER TIMESETTINGS - 2 |
SPECIAL MOVEMENT TIMESETTINGS | Front Panel Command: B.Timesetting No (e.g. B.5 accesses Special Movement Timesetting No 5) |
Timesetting No | Timesetting (Range: 0-5) | FUNCTION |
1 | 3.0 | SG 5 ALL RED (SUBSTITUTE E ALL RED) |
2 | 3.0 | SG 6 ALL RED (SUBSTITUTE E ALL RED) |
3 | 3.0 | SG 7 ALL RED (SUBSTITUTE C ALL RED) |
4 | 3.0 | SG 8 ALL RED (SUBSTITUTE C ALL RED) |
5 | 3.0 | SG 9 ALL RED (SUBSTITUTE C ALL RED) |
6 |  |  |
7 |  |  |
8 |  |  |
SPECIAL PURPOSE TIMESETTINGS | Front Panel Command: B.Timesetting No (e.g. B.19 accesses Special Movement Timesetting No 19)
Timesetting No | Timesetting (Range: 0-200) | FUNCTION |
9 | 4 | SG 5 SPECIAL MAXIMUM IN E (XSF 5) |  |
10 | 4 | SG 6 SPECIAL MAXIMUM IN E (XSF 6) |  |
11 | 4 | SG 7 & SG 9 SPECIAL MAXIMUM IN C (XSF 7) |  |
12 | 4 | SG 8 SPECIAL MAXIMUM IN C (XSF 8) |  |
13 | 15 | TIMER 1 : FOR HOLDING SG 5 RED IN A WITH P2 OPERATING |  |
14 | 4 | TIMER 2 : MINIMUM BLANK PERIOD FOR SG 5 IN A |  |
15 | 15 | P1 WALK TIME SUBSTITUTION IF CALLED BY WHEELCHAIR DET.17 |
16 | 15 | P2 WALK TIME SUBSTITUTION IF CALLED BY WHEELCHAIR DET.18 |
17 | 13 | P3 WALK TIME SUBSTITUTION IF CALLED BY WHEELCHAIR DET.19 |
18 | 0 | LIMIT GREEN WATCHDOG TIMER |  |
19 | 0 | SPECIAL FACILITY CONTROLS ALARM TIMER |  |
20 | 10 | ALL RED START UP INTERVAL |  |
21 | 14 | P4 WALK TIME SUBSTITUTION IF CALLED BY WHEELCHAIR DET.20 |
22 |  |  |  |
23 |  |  |  |
24 |  |  |  |
25 |  |  |  |
26 |  |  |  |
27 |  |  |  |
28 |  |  |  |
29 |  |  |  |
30 |  |  |  |
31 |  |  |  |
32 |  |  |  |
33 |  |  |  |
34 |  |  |  |
35 |  |  |  |
36 |  |  |  |
37 |  |  |  |
38 |  |  |  |
39 |  |  |  |
40 |  |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (CPG) |  | DATE | 18/08/10 |
G:\TMC Opsheets\Pending\[5607.htm]Controller 2 |