|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 3 |  |  |  |  |  |  |  |
SITE NAME | PRINCES HIGHWAY EAST NR SERVICE STREET | SITE NO. | 5655 |
DETECTOR FUNCTIONS |
| DETECTOR No. | Internal / External | Input number | SPECIAL FUNCTION | DETECTOR ALARMS |  |
| DA Category | Disable | DA on S/C only | Fault Simulation |
| Call & Extend | Call Only | Ignore |
| 1 | E | 1 | Call Ped 1** | 6 |  | P |  |  |  |  |  |
| 2 | E | 2 | Call Ped 2 | 6 |  | P |  |  |  |  |
| 3 |  |  |  | 1 |  |  |  |  |  |  |  |  |
| 4 |  |  |  | 1 |  |  |  |  |  |  |  |
| 5 | I | 1 | Extend SG1, Approach 1 * | 0 |  |  | P |  |  |  |
| 6 | I | 2 | Extend SG1, Approach 1 * | 0 |  |  | P |  |  |  |
| 7 | I | 3 | Extend SG2, Approach 2 * | 0 |  |  | P |  |  |  |
| 8 | I | 4 | Extend SG2, Approach 2 * | 0 |  |  | P |  |  |  |
| 9 | E | 5 | Off - Pelican POS; On - Normal POS | 1 | P |  |  |  |  |  |
| 10 |  |  |  |  |  |  |  |  |  |  |
| 11 |  |  |  |  |  |  |  |  |  |  |
| 12 |  |  |  |  |  |  |  |  |  |  |
| 13 |  |  |  |  |  |  |  |  |  |  |
| 14 |  |  |  |  |  |  |  |  |  |
| 15 |  |  |  |  |  |  |  |  |  |
| 16 |  |  |  |  |  |  |  |  |  |
| 17 |  |  |  |  |  |  |  |  |  |
| 18 |  |  |  |  |  |  |  |  |  |
| 19 |  |  |  |  |  |  |  |  |  |
| 20 |  |  |  |  |  |  |  |  |  |
|  | * For Queuing Feature, refer notes on page 6. |  |
|  | ** MSS11 is set for the duration of P1 demand. |  |
|  | MSS12 is set for the duration of P2 demand. |  |
INTERGREEN AND PEDESTRIAN TIMES |
|  | INTERGREEN TIMES |
|  |  | LEGAL SPEED | DESIGN SPEED | INTERGREEN |  |  |
|  |  | YELLOW | RED | YELLOW | RED | TOTAL |  |  |
|  | SG1 | 50 | 50 | - | 3.5 | 2.0 | 5.5 |  |  |  | TRUE |
|  | SG2 | 50 | 50 | - | 3.5 | 2.0 | 5.5 |  |
|  | PEDESTRIAN TIMES |  |  |  |  |
|  |  |  | WALK | CLEARANCE | MINIMUM SOLID DON'T WALK |  |
|  |  | DISTANCE (m) | TIME | DISTANCE (m) | TIME |
|  |  | GRAPH | ADOPTED | GRAPH | ADOPTED |
|  | P1 | 13.0 | 8 | 10 | 13.0 | 9 | 9 | 3.0 |  |  |  | 8 | 9 |
|  | P2 | 13.0 | 8 | 10 | 13.0 | 9 | 9 | 3.0 |  |  | 8 | 9 |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) | DATE | 30/06/15 |