|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 5 |  |
SITE NAME | PRINCES HIGHWAY EAST NR SERVICE STREET |  | SITE NO. | 5655 |
CONTROLLER TIMESETTINGS - 2 |
SPECIAL MOVEMENT TIMESETTINGS | Front Panel Command: B.Timesetting No (e.g. B.5 accesses Special Movement Timesetting No 5) |
Timesetting No | Timesetting (Range: 0-5) | FUNCTION |
1 | 2.0 | SG1 ALL RED (SUBSTITUTE B ALL RED) |  |
2 | 2.0 | SG2 ALL RED (SUBSTITUTE B ALL RED) |
3 |  |  |
4 |  |  |
5 |  |  |
6 |  |  |
7 |  |  |
8 |  |  |
SPECIAL PURPOSE TIMESETTINGS | Front Panel Command: B.Timesetting No (e.g. B.19 accesses Special Movement Timesetting No 19) |
Timesetting No | Timesetting (Range: 0-200) | FUNCTION |
9 | 16 | OFFSET T1 | LOW OFF PEAK No Z-, No Z+ |
10 | 16 | OFFSET T2 |
11 | 16 | OFFSET T1 | AM PEAK Z-, No Z+ |
12 | 16 | OFFSET T2 |
13 | 16 | OFFSET T1 | PM PEAK No Z-, Z+ |
14 | 16 | OFFSET T2 |
15 | 16 | OFFSET T1 | HIGH OFF PEAK Z-, Z+ |
16 | 16 | OFFSET T2 |
17 | 10 | SG1 ISOLATED MIN GREEN |  |
18 | 0 | LIMIT GREEN WATCHDOG TIMER | VC >= 4 ONLY |
19 | 0 | SPECIAL FACILITY CONTROLS ALARM TIMER |
20 | 10 | SG1 LINK MIN GREEN |  |
21 | 10 | SG2 ISOLATED MIN GREEN |  |
22 | 10 | SG2 LINK MIN GREEN |  |
23 |  |  |  |
24 |  |  |
25 | 25 | DELAY TIMER FOR APPROACH 2 QUEUING FEATURE |  |
26 | 10 | P1 WALK TIME SUBSTITUTION (XSF3 - MASTER / FLEXI) |  |
27 | 10 | P2 WALK TIME SUBSTITUTION (XSF3 - MASTER / FLEXI) |  |
28 |  |  |  |
29 |  |  |  |
30 |  |  |  |
31 |  |  |  |  |
32 |  |  |  |
33 |  |  |  |
34 |  |  |  |
35 |  |  |  |
36 |  |  |  |
37 |  |  |  |
38 |  |  |  |
39 |  |  |  |
40 |  |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) |  | DATE | 30/06/15 |