|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |
SITE NAME | PRINCES HIGHWAY EAST / BAILEY STREET | SITE NO. | 5657 |  |
DESIGN OF INTERGREEN AND PEDESTRIAN TIMES |  |
INTERGREEN TIMES |  |  |  |  |
PHASE | CLEARANCE DETAILS | LEGAL SPEED | DESIGN SPEED | INTERGREEN |  |  |
GROUP TRANSITION | DISTANCE | YELLOW | RED | YELLOW | RED | TOTAL |
A | 1 | g | P3 | 32.0 | 50 | 50 | 50 | 3.5 | 2.5 | 6.0 |  |  |  |
B | 4 | g | P2 | 21.0 | 50 | 50 | 50 | 3.5 | 1.5 | 5.0 |  |  |  |
C | 4 | g | P2 | 21.0 | 50 | 50 | 50 | 3.5 | 1.5 | 5.0 |  |  |  |
D |  | g |  |  |  |  |  |  |  |  |  |  |  |
E |  | g |  |  |  |  |  |  |  |  |  |  |  |
F |  | g |  |  |  |  |  |  |  |  |  |  |  |
G |  | g |  |  |  |  |  |  |  |  |  |  |  |
PHASE SPECIAL ALL REDS AND SPECIAL MOVEMENT ALL REDS |  |  |  |  |
FROM PHASE | TO PHASE | CLEARANCE DETAILS | DESIGN SPEED | ALL RED | PHASE or S.M. No* |  |  |  |
GROUP TRANSITION | DISTANCE |  |  |  |
B | C | 5 | g | 7 | 18.0 | 50 | 1.5 | - |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
C | B | 7 | g | P4 | 22.0 | 45 | 2.0 | C PHASE SPECIAL ALL RED |  |  |
|  |  | g |  |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |  |
* Specify where the timesetting is stored (the phase special all red or the special movement time setting number) |  |  |  |
PEDESTRIAN TIMES |  |  |
PED | PHASE(S) | WALK | CLEARANCE | MINIMUM SOLID DON'T WALK |  |  |
DISTANCE (m) | TIME | DISTANCE (m) | TIME |
GRAPH | ADOPTED | GRAPH | CL1 | CL2 |
1 | A |  | 15.0 | 15 | 14 | 9.0 | 6 | 6.0 |  | 6.0 |  |  | 6 |
2 | A |  | 15.0 | 15 | 14 | 9.0 | 6 | 6.0 |  | 6.0 |  |  | 9 |
3 | B |  | 13.0 | 8 | 10 | 13.0 | 9 | 9.0 |  | 5.0 |  |  | 5 |
4 | B |  | 13.0 | 8 | 10 | 13.0 | 9 | 9.0 |  | 5.0 |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
|  |  |  |  |  |  |  |  |  |  |  |  | #VALUE! |
DESIGNED BY: | [REDACTED] [REDACTED] (TW) | DATE | 3/07/15 |  |