|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 5 |  |
SITE NAME | PHE / MAFFRA - SALE ROAD | SITE NO. | 5610 |  |
DESIGN OF INTERGREEN AND PEDESTRIAN TIMES |  |
INTERGREEN TIMES |  |  |  |  |
PHASE | CLEARANCE DETAILS | LEGAL SPEED | DESIGN SPEED | INTERGREEN |  |
GROUP TRANSITION | DISTANCE | YELLOW | RED | YELLOW | RED | TOTAL |  |
A | 1 | g | P1 | 30.0 | 70 | 70 | 70 | 4.5 | 1.5 | 6.0 |  |
B | 5 | g | 1 | 23.0 | 70 | 70 | 45 | 4.5 | 2.0 | 6.5 |  |
C | 3 | g | 2 | 30.0 | 70 | 45 | 45 | 3.0 | 2.5 | 5.5 |  |
D | 5 | g | 1 | 23.0 | 70 | 45 | 45 | 3.0 | 2.0 | 5.0 |  |
E |  | g |  |  |  |  |  |  |  |  |  |
F |  | g |  |  |  |  |  |  |  |  |  |
G |  | g |  |  |  |  |  |  |  |  |  |
PHASE SPECIAL ALL REDS AND SPECIAL MOVEMENT ALL REDS |  |  |
FROM PHASE | TO PHASE | CLEARANCE DETAILS | DESIGN SPEED | ALL RED | PHASE or S.M. No* |  |
GROUP TRANSITION | DISTANCE |  |
|  |  | g |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |
|  |  | g |  |  |  |  |  |  |
* Specify where the timesetting is stored; the phase special all red or the special movement time setting number |  |  |
PEDESTRIAN TIMES |  |  |
PED | PHASE(S) | WALK | CLEARANCE | MINIMUM SOLID DON'T WALK |
DISTANCE (m) | TIME | DISTANCE (m) | TIME
GRAPH | ADOPTED | GRAPH | CL1 | CL2
P1 | C |  | 13.5 | 13 | 13 | 11.0 | 7 | 6.0 | 1.0 | 4.5 |
DESIGNED BY: | [REDACTED] [REDACTED] | DATE | 23-Apr-12 |  |
G:\TMC Opsheets\Pending\[5610.htm]Peds |  |