|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PAGE 4 |  |
SITE NAME | PRINCES HIGHWAY EAST / MACALISTER STREET | SITE NO. | 5607 |
APPROACH DEFINITIONS |
PHASE APPROACHES |  |  |  |
Approach No | EXTENDING DETECTORS | APPROACH TIMER AND TIMESETTING DEFINITION* | SIGNAL GROUP | APPROACH EXPIRY (EXPAP) | Refer Special Notes |
1 | 1, 2 | A11, B11 | 1 | A ↔ B |  |  |
2 | 4, 5 | A22 | 2 |  |  |  |
3 | 3 | B22, E11 | 5 |  |  |  |
4 | 7 | B33, D11, E33 | 3, 5 | B → D, D → E1, E2 |  |
5 | 9 | C11 | 7 |  |  |
6 | 12 | C22 | 8 |  |  |
7 | 8 | D22 | 3 |  |  |
8 | 10 | D33, E44 | 4, 6 | D → E1, E3 |  |
9 | 11 | D44 | 4 |  |  |
10 | 6 | E22 | 6 |  |  |
11 |  |  |  |  |  |
12 |  |  |  |  |  |
13 |  |  |  |  |  |
14 |  |  |  |  |  |
15 |  |  |  |  |  |
16 |  |  |  |  |  |
* There are 8 approach timers and 4 approach timesettings available per phase: |
- Where there are 4 or less approaches per phase, allocate one timesetting to each timer. |
For example: A11. A22, A33, B11, C11. |
- Where there are more than 4 approaches per phase, two or more timers must have the same timesetting. |
For example: A11. A21, A32, A43, A54, B11. |
SPECIAL APPROACHES |  |  |  |
Approach No | EXTENDING DETECTORS | APPROACH TIMESETTING | SIGNAL GROUP | DESCRIPTION | Refer Special Notes |
1 |  |  |  |  |  |
2 |  |  |  |  |  |
3 |  |  |  |  |  |
4 |  |  |  |  |  |
DESIGNED BY: | [REDACTED] [REDACTED] (CPG) | DATE | 18/08/10 |
G:\TMC Opsheets\Pending\[5607.htm]Approach |