|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | PELICAN |  |  | PAGE 3 |  |  |  |  |  |  |  |
SITE NAME | PHE BTW LYONS ST & HOOD ST | SITE NO. | 5611 |
DETECTOR FUNCTIONS |
| DETECTOR No. | Internal / External | SPECIAL FUNCTION | DETECTOR ALARMS |  |
| DA Category | Disable | DA on S/C only | Fault Simulation |
| Call & Extend | Call Only | Ignore |
| 1 | I | Extend SG1, Approach 1 * | 0 |  |  | P |  |  |  |  |
| 2 | I | Extend SG1, Approach 1 * | 0 |  |  | P |  |  |  |
| 3 | I | Extend SG2, Approach 2 * | 0 |  |  | P |  |  |  |  |  |
| 4 | I | Extend SG2, Approach 2 * | 0 |  |  | P |  |  |  |  |
| 5 | E | Call C. Places demand for Ped 1. | 6 |  | P |  |  |  |  |
| 6 | E | Off - Pelican POS; On - Normal POS | 1 | P |  |  |  |  |  |
| 7 |  |  |  |  |  |  |  |  |  |
| 8 |  |  |  |  |  |  |  |  |  |
| 9 |  |  |  |  |  |  |  |  |  |
| 10 |  |  |  |  |  |  |  |  |  |
| 11 |  |  |  |  |  |  |  |  |  |
| 12 |  |  |  |  |  |  |  |  |  |
| 13 |  |  |  |  |  |  |  |  |  |
| 14 |  |  |  |  |  |  |  |  |
| 15 |  |  |  |  |  |  |  |  |
|  | * For Queueing Feature, refer notes on page 6. |  |
INTERGREEN AND PEDESTRIAN TIMES |
|  | INTERGREEN TIMES |
|  |  | LEGAL SPEED | DESIGN SPEED | INTERGREEN |  |  |
|  |  | YELLOW | RED | YELLOW | RED | TOTAL |  |  |
|  | SG1 & SG2 | 60 | 60 | - | 4.0 | 2.0 | 6.0 |  |  |
|  | PEDESTRIAN TIMES |  |  |
|  |  |  | WALK | CLEARANCE | MINIMUM SOLID DON'T WALK |
|  |  | DISTANCE (m) | TIME | DISTANCE (m) | TIME |
|  |  | GRAPH | ADOPTED | GRAPH | ADOPTED |
|  | P1 | 18.0 | 8 | 8 | 18.0 | 12 | 12 | 3.0 |  |  | 8 | 12 |
DESIGNED BY: | [REDACTED] | DATE | 1/07/05 |
G:\TMC Opsheets\Pending\[5611.htm]Detectors |